# Raspberry Pi 4 Pi-hole Replica

- **Repo stack path:** `/home/fizzlepoof/repos/truenas-stacks/pihole/rpi4`
- **Suggested live stack path:** `~/pihole/stack`
- **Node role:** BACKUP2
- **Historical VIP target:** `10.5.30.53/24`

This node still needs its actual LAN IP confirmed before any future deployment.
The original Pi-hole HA design using `10.5.30.53` is retired; keep this only as historical/future-idea reference unless you intentionally build a new backup-DNS path.
Native keepalived config example is in `keepalived.conf.example`.
